{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"images":67},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":256,"n_cols":11,"rows_kept":256,"merged":[[1,0,9,0],[1,8,13,8],[1,9,9,9],[1,10,16,10],[10,0,13,0],[10,9,13,9],[14,0,16,0],[14,8,16,8],[14,9,16,9],[17,0,20,0],[17,8,20,8],[17,9,20,9],[17,10,20,10],[21,0,30,0],[21,8,22,8],[21,9,22,9],[21,10,22,10],[23,8,30,8],[23,9,30,9],[23,10,30,10],[31,0,35,0],[31,8,35,8],[31,9,35,9],[31,10,35,10],[36,0,43,0],[36,8,43,8],[36,9,43,9],[36,10,43,10],[44,0,48,0],[44,8,48,8],[44,9,48,9],[44,10,48,10],[49,0,53,0],[49,8,53,8],[49,9,53,9],[49,10,53,10],[54,0,64,0],[54,8,64,8],[54,9,57,9],[54,10,57,10],[58,9,64,9],[58,10,64,10],[65,0,92,0],[65,8,92,8],[65,9,86,9],[65,10,92,10],[87,9,92,9],[93,0,128,0],[93,8,128,8],[93,9,128,9],[93,10,128,10],[129,0,139,0],[129,8,139,8],[129,9,139,9],[129,10,139,10],[140,0,153,0],[140,8,153,8],[140,9,153,9],[140,10,152,10],[154,0,177,0],[154,8,177,8],[154,9,177,9],[154,10,177,10],[178,0,187,0],[178,8,187,8],[178,9,187,9],[178,10,187,10],[188,0,195,0],[188,8,195,8],[188,9,195,9],[188,10,195,10],[196,0,202,0],[196,8,202,8],[196,9,202,9],[196,10,202,10],[203,0,204,0],[203,8,206,8],[203,9,204,9],[203,10,204,10],[205,0,206,0],[205,9,206,9],[205,10,206,10],[207,0,210,0],[207,8,210,8],[207,9,210,9],[207,10,210,10],[211,0,216,0],[211,8,216,8],[211,9,216,9],[211,10,216,10],[217,0,219,0],[217,8,219,8],[217,9,219,9],[217,10,219,10],[220,0,221,0],[220,8,221,8],[224,0,225,0],[226,0,230,0],[226,8,230,8],[226,10,230,10],[231,0,238,0],[231,8,232,8],[231,9,232,9],[231,10,232,10],[233,8,238,8],[233,9,238,9],[233,10,238,10],[239,0,242,0],[239,8,244,8],[239,9,244,9],[239,10,244,10],[243,0,244,0],[245,0,247,0],[245,8,247,8],[245,10,247,10],[248,0,249,0],[248,8,249,8],[248,10,249,10],[250,0,253,0],[250,8,253,8],[250,9,251,9]]}
[null,"models","input voltage range","output voltage range","flow output","power","size","efficiency","highlight","drawing","photo"]
["CRPS series\nAC-DC","CRPS2361A","90VAC~264VAC/180VDC~300VDC","12V,+12Vsb ","28A","360W ","L185.0×W73.5× H40.0","gold","\"• Support black box write data\n• Support PMBus 1.2\n* Active PFC Power Factor Correction\n* Intel standard CRPS dimensions\n• Support FRU write data (embedded EEPROM)\n• Support N+N/N+1 redundancy\n• Support cold backup (live data sharing/online standby switching)\n• Support FW online update\n• Support reverse heat dissipation (independent model)\""]
[null,"CRPS550NZ","90VAC~264VAC/180VDC~300VDC","12V,+12Vsb ","45A","550W ","L185.0×W73.5× H40.0","Platinum"]
[null,"CRPS800BZ","90VAC~264VAC/180VDC~300VDC","12V,+12Vsb ","65A","800W ","L185.0×W73.5× H40.0","Platinum"]
[null,"CRPS800NC","90VAC~264VAC/180VDC~300VDC","12.2V ","65A","800W ","L185.0×W73.5× H40.0","Platinum+"]
[null,"CRPS1300AZ","90VAC~264VAC/180VDC~300VDC","12V,+12Vsb ","106.5A","1300W ","L185.0×W73.5× H40.0","Platinum"]
[null,"CRPS1600AZ","90VAC~264VAC/180VDC~300VDC","12V,+12Vsb ","132A","1600W ","L185.0×W73.5× H40.0","Platinum"]
[null,"CRPS2000AZ","90VAC~264VAC/180VDC~300VDC","12V,+12Vsb ","164A","2000W ","L185.0×W73.5× H40.0","Platinum+"]
[null,"CRPS2700A","90VAC~264VAC/180VDC~320VDC","54V,+12Vsb ","221A","3000W ","L185.0×W73.5× H40.0","Platinum+/ Titanium"]
[null,"CRPS3200A","90VAC~264VAC/180VDC~320VDC","54V,+12Vsb ","262.3A","3500W","L185.0×W73.5× H40.0"," Titanium"]
["CRPS AC-DC with china chip","CRPS550DZ","90Vac~264Vac/180Vdc~300Vdc","12V,+12Vsb ","45A","550W ","L185.0×W73.5× H40.0","Platinum"]
[null,"CRPS800DZ","90Vac~264Vac/180Vdc~300Vdc","12V,+12Vsb ","65A","800W ","L185.0×W73.5× H40.0","Platinum"]
[null,"CRPS1300DZ","90Vac~264Vac/180Vdc~300Vdc","12V,+12Vsb ","106.5A","1300W ","L185.0×W73.5× H40.0","Platinum"]
[null,"CRPS1600DZ","90Vac~264Vac/180Vdc~300Vdc","12V,+12Vsb","132A","1600W ","L185.0×W73.5× H40.0","Platinum"]
["CRPS DC-DC","CRPSD550NZ","36V~75V","12V,+12Vsb","45A","550W ","L185.0×W73.5× H40.0","Platinum","• Efficiency up to 92%\n• Low ripple and output noise、\n• High reliability\n* Input overvoltage protection\n• Output overvoltage protection"]
[null,"CRPSD800BZ","36V~75V","12V,+12Vsb","65A","800W ","L185.0×W73.5× H40.0","Platinum"]
[null,"CRPSD1300AZ","36V~75V","12V,+12Vsb","106.5A","1300W ","L185.0×W73.5× H40.0","Platinum"]
["CRPSH series","CRPSH3080",null,"12V/3.3V/5V/5Vsb/-12V ",null,"800W ","225x77.5x83.8",null,"• Cable specifications can be customized\n• High conversion efficiency\n* Input undervoltage protection\n• Overcurrent and short circuit protection\n• Overheating protection\n• Input and output isolation\n• Metal bottom plate, fully enclosed housing"]
[null,"CRPSH1200A",null,"12V/3.3V/5V/5Vsb/-12V",null,"1200W","225x77.5x83.8"]
[null,"CRPSH1600A",null,"12V/3.3V/5V/5Vsb/-12V",null,"1600W","225x77.5x83.8"]
[null,"CRPSH2000A",null,"12V/3.3V/5V/5Vsb/-12V",null,"2000W","225x77.5x83.8"]
["SLIM  series","SLIMG2151A","100-240Vac","12V,+12Vsb",null,"150W","L164.5×W50.5×H40mm",null,"Active Power Factor Correction\n•Support 1+1/N+1 redundancy\n•Input signal 90-264VAC\n•Efficiency more than 88%\n*EMC complies with EN55032 ClassB\n"]
[null,"SLIMG2151A","100-240Vac","12V,+12Vsb",null,"200W","L164.5×W50.5×H40mm"]
[null,"SLIM200A ","100-240Vac","12V,+12Vsb ",null,"200W ","195x50.5x40",null,"• Cable specifications can be customized\n•Conversion efficiency\n*Input undervoltage protection\n•Overcurrent and short circuit protection\n•Overheating protection\n•Input and output isolation\n•Integrated PCB mounting\n•Metal bottom plate, fully enclosed housing"]
[null,"SLIM300A ","100-240Vac","12V,+12Vsb ",null,"300W ","195x50.5x40"]
[null,"SLIM450A ","100-240Vac","12V,+12Vsb ",null,"450W ","220x50.0x40"]
[null,"SLIM650A ","100-240Vac","12V,+12Vsb ",null,"650W ","220x50.0x40"]
[null,"SLIM1200A ","100-240Vac","12V,+12Vsb ",null,"1200W ","321x54.5x40"]
[null,"SLIM1300A ","100-240Vac","12V,+12Vsb ",null,"1300W ","321x54.5x40"]
[null,"SLIM1600A ","100-240Vac","12V,+12Vsb ",null,"1600W ","360x50.0x40"]
[null,"SLIM2000A ","100-240Vac","12V,+13Vsb",null,"2000W","360x54.5x40"]
["ATX  series","ATXG5251A ","100-240Vac","12V/3.3V/5V/5Vsb/-12V ",null,"250W ","150x140x86","90+","Active Power Factor Correction\n•Intelligent Fan Speed ​​Control\n•Environmental Standard: RoHS\n•EMI/RFI: CISPR22; CLASS B\n•Protection: OVP, OCP, OTP, SCP\n•Safety: CCC\n•Cable Specifications on request"]
[null,"ATXG5401A ","100-240Vac","12V/3.3V/5V/5Vsb/-12V ",null,"400W ","150x140x86","90+"]
[null,"ATXG5501A ","100-240Vac","12V/3.3V/5V/5Vsb/-12V ",null,"500W ","150x140x86","90+"]
[null,"ATXG5601A ","100-240Vac","12V/3.3V/5V/5Vsb/-12V ",null,"600W ","150x140x86","90+"]
[null,"ATXG5701A ","100-240Vac","12V/3.3V/5V/5Vsb/-12V ",null,"700W","150x140x86","90+"]
["TFX  series","TFXH5181A ","180-264Vac","12V/3.3V/5V/5Vsb/-12V ",null,"180W ","175.5x85x65","75+","•80PLUSBronze\n•Active Power Factor Correction\n•Intelligent Fan Speed ​​Control\n•Environmental Standards: RoHS, WEEE, REACH\n•Application: Industrial\n•EMI/RFI: CISPR22; CLASS B\n•Protection: OVP, OCP, OTP, SCP\n•Safety: CCC, FCC, UL, CUL, CE, BSMI, CB, EMC"]
[null,"TFXB2181A ","180-264Vac","12V/5Vsb ",null,"180W","150x85x65","85+"]
[null,"TFXH5201A ","180-264Vac","12V/3.3V/5V/5Vsb/-12V ",null,"200W ","175.5x85x65","75+"]
[null,"TFXB2201A ","180-264Vac","12V/5Vsb ",null,"200W ","150x85x65","85+"]
[null,"TFXH5251A ","180-264Vac","12V/3.3V/5V/5Vsb/-12V ",null,"250W ","175.5x85x65","75+"]
[null,"TFXG5251B ","180-264Vac","12V/3.3V/5V/5Vsb/-12V ",null,"250W ","175.5x85x65","90+"]
[null,"TFXB2261A ","180-264Vac","12V/5Vsb ",null,"260W ","150x85x65","85+"]
[null,"TFXB2301A ","180-264Vac","12V/5Vsb ",null,"300W","150x85x65","85+"]
["FLEX series","FLEXG5250A ","100-240Vac.","12V/3.3V/5V/5Vsb/-12V ",null,"250W ","150x81.5x40.5","90+","• Wide input range\n• Conversion efficiency\n* Input undervoltage protection\n• Overcurrent and short circuit protection\n• Overtemperature protection\n• Input and output isolation\n• Integrated PCB mounting\n• Metal bottom plate, fully enclosed case"]
[null,"FLEXG5400A ","100-240Vac.","12V/3.3V/5V/5Vsb/-12V ",null,"400W ","150x81.5x40.5","90+"]
[null,"FLEXG5500A ","100-240Vac.","12V/3.3V/5V/5Vsb/-12V ",null,"500W ","150x81.5x40.5","90+"]
[null,"FLEXG5600A ","180-264Vac","12V/3.3V/5V/5Vsb/-12V ",null,"600W ","150x81.5x40.5","90+"]
[null,"FLEXG5700A ","180-264Vac","12V/3.3V/5V/5Vsb/-12V ",null,"700W","150x81.5x40.5","90+"]
["DC-DC\nbrick","ZYDF600H-110S**","43~160VDC","12~48V",null,"600W","brick",{"v":0.9,"d":"90%"},"Wide input range\nHigh conversion efficiency\nInput undervoltage protection\nOvercurrent, short circuit protection\nOverheating protection\nInput and output isolation\nIntegrated PCB installation\nMetal bottom plate, fully enclosed body\nRemote control and remote compensation, output voltage regulation"]
[null,"ZYDF1200H-280S12","240~280VDC","12V",null,"1200W ","brick",{"v":0.935,"d":"93.50%"}]
[null,"ZYDF1300H-48S28","36~75VDC","28V ",null,"1300W","brick",{"v":0.95,"d":"95%"}]
[null,"ZYDF1500-280S12","240~280VDC","12V",null,"1500W","brick",{"v":0.94,"d":"94%"}]
[null,"ZYDF2000H-540S28","400~800VDC","28V",null,"2000W","brick",{"v":0.96,"d":"96%"}]
["DC-DC F series（brick）","ZYDF600-110S24 ","66-160Vdc","24V ",null,"600W ","brick",{"v":0.91,"d":"91%"},"• Wide input signal range\n•High conversion efficiency\n*Input undervoltage protection\n•Overcurrent and short circuit protection\n•Overheating protection\n•Input and output isolation\n•Integrated PCB mounting\n•Metal bottom plate, fully enclosed housing"]
[null,"ZYDF600-110S28 ","66-160Vdc","28V ",null,"600W ","brick",{"v":0.91,"d":"91%"}]
[null,"ZYDF600-110S36 ","66-160Vdc","36V ",null,"600W ","brick",{"v":0.91,"d":"91%"}]
[null,"ZYDF600-110S48 ","66-160Vdc","48V ",null,"600W ","brick",{"v":0.92,"d":"92%"}]
[null,"ZYDF1200-280S12 ","200-425Vdc","12V ",null,"1200W ","brick",{"v":0.95,"d":"95%"}]
[null,"ZYDF1200-280S28 ","200-425Vdc","28V ",null,"1200W ","brick",{"v":0.95,"d":"95%"}]
[null,"ZYDF1300-48S28 ","36-75Vdc","28V ",null,"1300W ","brick",{"v":0.95,"d":"95%"}]
[null,"ZYDF1300-48S50 ","36-75Vdc","50V ",null,"1300W ","brick",{"v":0.95,"d":"95%"}]
[null,"ZYDF1500-280S12 ","200-425Vdc","12V ",null,"1500W ","brick",{"v":0.95,"d":"95%"}]
[null,"ZYDF1500-280S28 ","200-425Vdc","28V ",null,"1500W ","brick",{"v":0.95,"d":"95%"}]
[null,"ZYDF2000-540S28 ","400-800Vdc","28V ",null,"2000W","brick",{"v":0.95,"d":"95%"}]
["DC-DC H series （1/2 brick）","ZYDH1300H-48S**","36~75VDC","28~50V",null,"1300W","1/2brick",{"v":0.95,"d":"95%"},"• Wide input signal range\n•High conversion efficiency\n*Input undervoltage protection\n•Overcurrent and short circuit protection\n•Overheating protection\n•Input and output isolation\n•Integrated PCB mounting\n•Metal bottom plate, fully enclosed housing"]
[null,"ZYDH1500H-48S50","36~75VDC","50V",null,"1500W","1/2brick",{"v":0.95,"d":"95%"}]
[null,"ZYDH75-24S12 ","18-36Vdc","12V ",null,"75W ","1/2brick",{"v":0.89,"d":"89%"}]
[null,"ZYDH100-24S05 ","18-36Vdc","5V ",null,"100W ","1/2brick",{"v":0.89,"d":"89%"}]
[null,"ZYDH200-110S05 ","43-160Vdc","5V ",null,"200W ","1/2brick",{"v":0.89,"d":"89%"}]
[null,"ZYDH300-24S12 ","18-36Vdc","12V ",null,"300W ","1/2brick",{"v":0.89,"d":"89%"}]
[null,"ZYDH300-24S15 ","18-36Vdc","15V ",null,"300W ","1/2brick",{"v":0.89,"d":"89%"}]
[null,"ZYDH300-24S24 ","18-36Vdc","24V ",null,"300W ","1/2brick",{"v":0.89,"d":"89%"}]
[null,"ZYDH300-24S28 ","18-36Vdc","28V ",null,"300W ","1/2brick",{"v":0.89,"d":"89%"}]
[null,"ZYDH300-24S48 ","18-36Vdc","48V ",null,"300W ","1/2brick",{"v":0.89,"d":"89%"}]
[null,"ZYDH300-48S48 ","36-75Vdc","48V ",null,"300W ","1/2brick",{"v":0.89,"d":"89%"}]
[null,"ZYDH300-110S12 ","43-160Vdc","12V ",null,"300W ","1/2brick",{"v":0.89,"d":"89%"}]
[null,"ZYDH300-110S14 ","43-160Vdc","14V ",null,"300W ","1/2brick",{"v":0.89,"d":"89%"}]
[null,"ZYDH300-110S15 ","43-160Vdc","15V ",null,"300W ","1/2brick",{"v":0.89,"d":"89%"}]
[null,"ZYDH300-110S24 ","43-160Vdc","24V ",null,"300W ","1/2brick",{"v":0.89,"d":"89%"}]
[null,"ZYDH300-110S24C ","43-160Vdc","24V ",null,"300W ","1/2brick",{"v":0.89,"d":"89%"}]
[null,"ZYDH300-110S36 ","43-160Vdc","36V ",null,"300W ","1/2brick",{"v":0.89,"d":"89%"}]
[null,"ZYDH300-280S28C ","185-400Vdc","28V ",null,"300W","1/2brick",{"v":0.91,"d":"91%"}]
[null,"ZYDH300-280S48C ","185-400Vdc","48V ",null,"300W ","1/2brick",{"v":0.91,"d":"91%"}]
[null,"ZYDH350-48S28 ","36-75Vdc","28V ",null,"350W ","1/2brick",{"v":0.91,"d":"91%"}]
[null,"ZYDH350-24S48 ","18-36Vdc","48V ",null,"350W ","1/2brick",{"v":0.91,"d":"91%"}]
[null,"ZYDH400-110S48 ","66-160Vdc","48V ",null,"400W ","1/2brick",{"v":0.91,"d":"91%"}]
[null,"ZYDH1000-48S28 ","36-75Vdc","28V ",null,"1000W ","1/2brick",{"v":0.95,"d":"95%"}]
[null,"ZYDH1000-48S48 ","36-75Vdc","48V ",null,"1000W ","1/2brick",{"v":0.95,"d":"95%"}]
[null,"ZYDH1000-270S12 ","200-425Vdc","12V ",null,"1000W ","1/2brick",{"v":0.95,"d":"95%"}]
[null,"ZYDH1000-270S28 ","200-425Vdc","28V ",null,"1000W ","1/2brick",{"v":0.95,"d":"95%"}]
[null,"ZYDH1200-540S12 ","400-800Vdc","12V ",null,"1200W ","1/2brick",{"v":0.95,"d":"95%"}]
[null,"ZYDH1200-540S28 ","400-800Vdc","28V ",null,"1200W","1/2brick",{"v":0.95,"d":"95%"}]
["DC-DC\n1/4brick   series Q","ZYDQ50-110S12 ","43-160V","12V ",null,"50W ","1/4brick",{"v":0.92,"d":"92%"},"• Wide input signal range\n•High conversion efficiency\n*Input undervoltage protection\n•Overcurrent and short circuit protection\n•Overheating protection\n•Input and output isolation\n•Integrated PCB mounting\n•Metal bottom plate, fully enclosed housing"]
[null,"ZYDQ60-110S12 ","18-160V","12V ",null,"60W ","1/4brick",{"v":0.92,"d":"92%"}]
[null,"ZYDQ75-110S05 ","43-160V","5V ",null,"75W ","1/4brick",{"v":0.92,"d":"92%"}]
[null,"ZYDQ100-110S05 ","36-75V","5V ",null,"100W ","1/4brick",{"v":0.92,"d":"92%"}]
[null,"ZYDQ100-110S12 ","43-160V","12V ",null,"100W ","1/4brick",{"v":0.92,"d":"92%"}]
[null,"ZYDQ100-48S96 ","43-160V","96V ",null,"100W ","1/4brick",{"v":0.92,"d":"92%"}]
[null,"ZYDQ120-24S12 ","9-36V","12V ",null,"120W ","1/4brick",{"v":0.92,"d":"92%"}]
[null,"ZYDQ150-24S15 ","18-36V","15V ",null,"150W ","1/4brick",{"v":0.92,"d":"92%"}]
[null,"ZYDQ150-24S19 ","18-36V","19V ",null,"150W ","1/4brick",{"v":0.92,"d":"92%"}]
[null,"ZYDQ150-24S24 ","18-36V","24V ",null,"150W ","1/4brick",{"v":0.92,"d":"92%"}]
[null,"ZYDQ150-24S28 ","18-36V","28V ",null,"150W ","1/4brick",{"v":0.92,"d":"92%"}]
[null,"ZYDQ150-24S36 ","9-36V","36V ",null,"150W ","1/4brick",{"v":0.92,"d":"92%"}]
[null,"ZYDQ150-24S48 ","9-36V","48V ",null,"150W ","1/4brick",{"v":0.92,"d":"92%"}]
[null,"ZYDQ150-48S12 ","36-75V","12V ",null,"150W ","1/4brick",{"v":0.92,"d":"92%"}]
[null,"ZYDQ150-48S28 ","36-75V","28V ",null,"150W","1/4brick",{"v":0.92,"d":"92%"}]
[null,"YDQ150-110S12 ","43-160V","12V ",null,"150W ","1/4brick",{"v":0.92,"d":"92%"}]
[null,"ZYDQ150-110S15 ","43-160V","15V ",null,"150W ","1/4brick",{"v":0.92,"d":"92%"}]
[null,"ZYDQ150-110S24T ","43-160V","24V ",null,"150W ","1/4brick",{"v":0.92,"d":"92%"}]
[null,"ZYDQ150-110S36 ","43-160V","36V ",null,"150W ","1/4brick",{"v":0.92,"d":"92%"}]
[null,"ZYDQ150-110S48 ","43-160V","48V ",null,"150W ","1/4brick",{"v":0.92,"d":"92%"}]
[null,"ZYDQ150-110S110 ","43-160V","110V ",null,"150W ","1/4brick",{"v":0.92,"d":"92%"}]
[null,"ZYDQ225-48S15 ","36-75V","15V ",null,"225W ","1/4brick",{"v":0.92,"d":"92%"}]
[null,"ZYDQ600-48S12 ","36-75Vdc","12V ",null,"600W ","1/4brick",{"v":0.95,"d":"95%"}]
[null,"ZYDQ700-48S28 ","36-75Vdc","28V ",null,"700W ","1/4brick",{"v":0.95,"d":"95%"}]
[null,"ZYDQ750-380S12 ","330-400Vdc","12V ",null,"750W ","1/4brick",{"v":0.95,"d":"95%"}]
[null,"ZYDQ800-380S12 ","330-400Vdc","12V ",null,"800W ","1/4brick",{"v":0.95,"d":"95%"}]
[null,"ZYDQ1000-48S12 ","40-60Vdc","12V ",null,"1000W ","1/4brick",{"v":0.95,"d":"95%"}]
[null,"ZYDQ1300-54S12 ","40-60Vdc","12V ",null,"1300W ","1/4brick",{"v":0.95,"d":"95%"}]
[null,"ZYDQ1500-54S12 ","40-60Vdc","12V ",null,"1500W ","1/4brick",{"v":0.95,"d":"95%"}]
[null,"ZYDQ1600-54S12 ","40-60Vdc","12V ",null,"1600W","1/4brick",{"v":0.95,"d":"95%"}]
[null,"ZYDQ200-110S24","43~160VDC","24V",null,"200W","1/4brick",{"v":0.9,"d":"90%"}]
[null,"ZYDQ200-280S**","180~425VDC","12~15V",null,"200W","1/4brick",{"v":0.9,"d":"90%"}]
[null,"ZYDQ250-280S**","180~425VDC","15~24V",null,"250W","1/4brick",{"v":0.91,"d":"91%"}]
[null,"ZYDQ750-54S12","36~75VDC","12V",null,"750W","1/4brick",{"v":0.962,"d":"96.20%"}]
[null,"ZYDQ1200-380S12","360~400VDC","12V",null,"1200W","1/4brick",{"v":0.971,"d":"97.10%"}]
[null,"ZYDQ2000-380S48","340~400VDC","42.5~50V",null,"2000W","1/4brick",{"v":0.973,"d":"97.30%"}]
["DC-DC\n1/8brick  series","ZYDE120-48S12 ","36-75Vdc","12V ",null,"120W ","1/8brick",{"v":0.93,"d":"93.00%"},"• Wide input voltage range: high conversion efficiency of 2:1\n•Input undervoltage protection\n•Overcurrent and short circuit protection\n•Overtemperature protection\n•Input and output isolation\n•Integrated PCB mounting\n•Metal bottom plate, fully enclosed housing"]
[null,"ZYDE200-48S05 ","36-75Vdc","5V ",null,"200W ","1/8brick",{"v":0.91,"d":"91.00%"}]
[null,"ZYDE400-48S12 ","36-75Vdc","12V ",null,"400W","1/8brick",{"v":0.95,"d":"95%"}]
[null,"ZYDE75-48S05","36~75VDC","5V",null,"75W","1/8brick",{"v":0.92,"d":"92%"}]
[null,"ZYDE100-48S05","36~75VDC","5V",null,"100W","1/8brick",{"v":0.92,"d":"92%"}]
[null,"ZYDE120-48S05","36~75VDC","5V",null,"120W","1/8brick",{"v":0.91,"d":"91%"}]
[null,"ZYDE150-48S05","36~75VDC","5V",null,"150W","1/8brick",{"v":0.92,"d":"92%"}]
[null,"ZYDE200-48S**","36~75VDC","5~12V",null,"200W","1/8brick",{"v":0.93,"d":"93%"}]
[null,"ZYDE240-48S12","36~75VDC","12V",null,"240W","1/8brick",{"v":0.93,"d":"93%"}]
[null,"ZYDE300-48S**","36~75VDC","12~28V",null,"300W","1/8brick",{"v":0.95,"d":"95%"}]
[null,"ZYDE400-48S12","36~75VDC","12V",null,"400W","1/8brick",{"v":0.95,"d":"95%"}]
["DC-DC \n1*1 series","ZYDZ15-24S**","9~36VDC","3.3~12V",null,"15W","1/8brick",{"v":0.81,"d":"81%"},"• Wide input signal range\n•High conversion efficiency\n•Input undervoltage protection\n•Overcurrent and short circuit protection\n•Overheating protection\n•Input and output isolation\n•Integrated PCB mounting\n•Metal bottom plate, fully enclosed housing"]
[null,"ZYDZ15-110S**","43~160VDC","15~48V",null,"15W","1/8brick",{"v":0.84,"d":"84%"}]
[null,"ZYDZ10-24S05 ","18-36V","5V ",null,"10W ","1\"x1\"",{"v":0.81,"d":"81%"}]
[null,"ZYDZ10-24S12 ","18-36V","12V ",null,"10W ","1\"x1\"",{"v":0.81,"d":"81%"}]
[null,"ZYDZ10-24S15 ","18-36V","15V ",null,"10W ","1\"x1\"",{"v":0.81,"d":"81%"}]
[null,"ZYDZ10-24S24 ","18-36V","24V ",null,"10W ","1\"x1\"",{"v":0.81,"d":"81%"}]
[null,"ZYDZ15-24S05 ","18-36V","5V ",null,"15W ","1\"x1\"",{"v":0.81,"d":"81%"}]
[null,"ZYDZ15-24S12 ","18-36V","12V ",null,"15W ","1\"x1\"",{"v":0.81,"d":"81%"}]
[null,"ZYDZ15-24S15 ","18-36V","15V ",null,"15W ","1\"x1\"",{"v":0.81,"d":"81%"}]
[null,"ZYDZ15-24S24 ","18-36V","24V ",null,"15W","1\"x1\"",{"v":0.84,"d":"84%"}]
[null,"ZYDZ15-110S05 ","43-160V","5V ",null,"15W","1\"x1\"",{"v":0.84,"d":"84%"}]
[null,"ZYDZ15-110S12 ","43-160V","12V ",null,"15W","1\"x1\"",{"v":0.84,"d":"84%"}]
[null,"ZYDZ15-110S15 ","43-160V","15V ",null,"15W","1\"x1\"",{"v":0.84,"d":"84%"}]
[null,"ZYDZ15-110S24 ","43-160V","24V ",null,"15W","1\"x1\"",{"v":0.84,"d":"84%"}]
["DC-DC 2*1 series","ZYDX15-48S05D ","18-75V","5V ",null,"15W ","2\"x1\"(Narrow angle of inclination) ",{"v":0.85,"d":"85%"},"• Wide input signal range\n•High conversion efficiency\n•Input undervoltage protection\n•Overcurrent and short circuit protection\n•Overheating protection\n•Input and output isolation\n•Integrated PCB mounting\n•Metal bottom plate, fully enclosed housing"]
[null,"ZYDX15-110S05 ","43-160V","5V ",null,"15W ","2\"x1\"(Narrow angle of inclination) ",{"v":0.83,"d":"83%"}]
[null,"ZYDX15-110S12 ","43-160V","12V ",null,"15W ","2\"x1\"(Narrow angle of inclination) ",{"v":0.85,"d":"85%"}]
[null,"ZYDX40-12S28 ","9-36V ","28V",null,"40W ","2\"x1\"(wide tilt angle)",{"v":0.88,"d":"88%"}]
[null,"ZYDX60-24S05 ","9-36V ","5V",null,"60W ","2\"x1\"(wide tilt angle)",{"v":0.87,"d":"87%"}]
[null,"ZYDX60-24S12 ","18-36V ","12V",null,"60W ","2\"x1\"(wide tilt angle)",{"v":0.88,"d":"88%"}]
[null,"ZYDX60-24S24 ","18-36V ","24V",null,"60W","2\"x1\"(wide tilt angle)",{"v":0.87,"d":"87%"}]
[null,"ZYDX60-24S36 ","18-36V ","36V ",null,"60W","2\"x1\"(wide tilt angle)",{"v":0.87,"d":"87%"}]
[null,"ZYDX60-24S48 ","18-36V ","48V ",null,"60W","2\"x1\"(wide tilt angle)",{"v":0.87,"d":"87%"}]
[null,"ZYDX60-48S48 ","36-75V ","48V ",null,"60W","2\"x1\"(wide tilt angle)",{"v":0.87,"d":"87%"}]
[null,"ZYDX60-110S03 ","43-160V ","3.3V",null,"60W","2\"x1\"(wide tilt angle)",{"v":0.86,"d":"86%"}]
[null,"ZYDX60-110S05 ","43-160V ","5V",null,"60W","2\"x1\"(wide tilt angle)",{"v":0.86,"d":"86%"}]
[null,"ZYDX60-110S12 ","43-160V ","12V",null,"60W","2\"x1\"(wide tilt angle)",{"v":0.87,"d":"87%"}]
[null,"ZYDX60-110S15 ","43-160V ","15V ",null,"60W","2\"x1\"(wide tilt angle)",{"v":0.87,"d":"87%"}]
[null,"ZYDX60-110S24 ","43-160V ","24V",null,"60W","2\"x1\"(wide tilt angle)",{"v":0.87,"d":"87%"}]
[null,"ZYDX60-110S36 ","43-160V ","36V ",null,"60W","2\"x1\"(wide tilt angle)",{"v":0.86,"d":"86%"}]
[null,"ZYDX60-110S48 ","43-160V ","48V ",null,"60W","2\"x1\"(wide tilt angle)",{"v":0.89,"d":"89%"}]
[null,"ZYDX40-12S28A","9~36VDC","±28V",null,"40W","2\"x1\"(wide tilt angle)",{"v":0.88,"d":"88%"}]
[null,"ZYDX40-24D**","9~40VDC","±12~36V",null,"40W","2\"x1\"(wide tilt angle)",{"v":0.88,"d":"88%"}]
[null,"ZYDX40-110D**","43~160VDC","±12~15V",null,"40W","2\"x1\"(wide tilt angle)",{"v":0.88,"d":"88%"}]
[null,"ZYDX15-24S**","9~36VDC","5~12V",null,"15W","2\"x1\"(Narrow angle of inclination) ",{"v":0.86,"d":"86%"}]
[null,"ZYDX15-48S**","18~75VDC","5~12V",null,"15W","2\"x1\"(Narrow angle of inclination) ",{"v":0.86,"d":"86%"}]
[null,"ZYDX15-110S**","18~160VDC","5~12V",null,"15W","2\"x1\"(Narrow angle of inclination) ",{"v":0.85,"d":"85%"}]
[null,"ZYDX20-110S24","43~160VDC","24V",null,"20W","2\"x1\"(Narrow angle of inclination) ",{"v":0.86,"d":"86%"}]
["AC-DC 4*2 without without housing","ZYAD100-220S12","90~264VAC","12V",null,"100W","4\"×2\"",{"v":0.89,"d":"89%"},"• Wide input signal range\n•High conversion efficiency\n•Input undervoltage protection\n•Overcurrent and short circuit protection\n•Overheating protection\n•Input and output isolation\n•Integrated PCB mounting\n•Metal bottom plate, fully enclosed housing\n"]
[null,"ZYAD100-220S15","90~264VAC","15V ",null,"100W","4\"×2\"",{"v":0.89,"d":"89%"}]
[null,"ZYAD100-220S24","90~264VAC","24V",null,"100W","4\"×2\"",{"v":0.9,"d":"90%"}]
[null,"ZYAD100-220S28","90~264VAC","28V",null,"100W","4\"×2\"",{"v":0.9,"d":"90%"}]
[null,"ZYAD100-220S48","90~264VAC","48V",null,"100W","4\"×2\"",{"v":0.91,"d":"91%"}]
[null,"ZYAD225-220S12","90~264VAC","12V",null,"225W","4\"×2\"",{"v":0.92,"d":"92%"}]
[null,"ZYAD225-220S15","90~264VAC","15V",null,"225W","4\"×2\"",{"v":0.93,"d":"93%"}]
[null,"ZYAD225-220S24","90~264VAC","24V",null,"225W","4\"×2\"",{"v":0.94,"d":"94%"}]
[null,"ZYAD225-220S28","90~264VAC","28V",null,"225W","4\"×2\"",{"v":0.94,"d":"94%"}]
[null,"ZYAD225-220S48","90~264VAC","48V",null,"225W","4\"×2\"",{"v":0.94,"d":"94%"}]
["AC-DC 1/2brick series","ZYAH200-220S12","90~264VAC","12V",null,"200W","1/2brick",{"v":0.85,"d":"85%"},"Wide input range\nHigh conversion efficiency\nInput undervoltage protection\nOvercurrent, short circuit protection\nOverheating protection\nInput and output isolation\nIntegrated PCB installation\nMetal bottom plate, fully enclosed body\nRemote control and remote compensation, output voltage regulation"]
[null,"ZYAH200-220S15","90~264VAC","15V ",null,"200W","1/2brick",{"v":0.85,"d":"85%"}]
[null,"ZYAH200-220S24","90~264VAC","24V",null,"200W","1/2brick",{"v":0.86,"d":"86%"}]
[null,"ZYAH200-220S28","90~264VAC","28V",null,"200W","1/2brick",{"v":0.86,"d":"86%"}]
[null,"ZYAH200-220S48","90~264VAC","48V",null,"200W","1/2brick",{"v":0.86,"d":"86%"}]
[null,"ZYAH300-220S12","90~264VAC","12V",null,"300W","1/2brick",{"v":0.86,"d":"86%"}]
[null,"ZYAH350-220S24","90~264VAC","24V",null,"350W","1/2brick",{"v":0.86,"d":"86%"}]
[null,"ZYAH350-220S48","90~264VAC","48V",null,"350W","1/2brick",{"v":0.86,"d":"86%"}]
["AC-DC brick series","ZYAF510-220S12","90~264VAC","12V",null,"510W","brick",{"v":0.91,"d":"91%"},"Wide input range\nHigh conversion efficiency\nInput undervoltage protection\nOvercurrent, short circuit protection\nOverheating protection\nInput and output isolation\nIntegrated PCB installation\nMetal bottom plate, fully enclosed body\nRemote control and remote compensation, output voltage regulation\n"]
[null,"ZYAF510-220S2","90~264VAC","24V",null,"510W","brick",{"v":0.92,"d":"92%"}]
[null,"ZYAF510-220S30","90~264VAC","30V",null,"510W","brick",{"v":0.92,"d":"92%"}]
[null,"ZYAF510-220S48","90~264VAC","48V",null,"510W","brick",{"v":0.92,"d":"92%"}]
[null,"ZYAF700-220S12","90~264VAC","12V",null,"700W","brick",{"v":0.92,"d":"92%"}]
[null,"ZYAF700-220S24","90~264VAC","24V",null,"700W","brick",{"v":0.92,"d":"92%"}]
[null,"ZYAF700-220S48","90~264VAC","48V",null,"700W","brick",{"v":0.92,"d":"92%"}]
["AC-DC F series","ZYAF1000-220S28 ","100-240Vac","28V ",null,"1000W ","116.8x61.0x13.3",{"v":0.91,"d":"91%"},"• Wide input signal range\n• High conversion efficiency\n* Input undervoltage protection\n• Overcurrent and short circuit protection\n• Overheating protection\n• Input and output isolation\n• Integrated PCB mounting\n• Metal bottom plate, fully enclosed housing"]
[null,"ZYAF1000-220S48 ","85-265Vac","48V ",null,"1000W","116.8x61.0x13.3",{"v":0.91,"d":"91%"}]
["AC-DC H series","ZYAH500-220S12 ","85-265Vac","12V ",null,"500W ","110.8x50.8x13.7mm",{"v":0.92,"d":"92%"}]
[null,"ZYAH500-220S28 ","85-265Vac","28V ",null,"500W","110.8x50.8x13.7mm",{"v":0.92,"d":"92%"}]
["AC-DC quick install ","ZYAV200-220S24 ","165-265V","24V ",null,"200W ","EOL",null,"•Natural cooling and heat dissipation\n•Output power 100-800 W\n•Module terminal type\n•Hexagonal metal shield\n•Easy installation"]
[null,"ZYAV300-220S48 ","165-265V","48V ",null,"300W ","EOL"]
[null,"ZYAV500-220S48 ","165-265V","48V ",null,"500W ","EOL"]
[null,"ZYAV800-220S48 ","165-265V","48V ",null,"800W","EOL"]
["DC-DC quick install","ZYDV100-24S05 ","18-36V","5V ",null,"100W ","EOL",null,"•Natural cooling and heat dissipation\n• Output power 100-500 W\n• Hexagonal metal shield\n•Module terminal type\n•Easy installation\n• Small size"]
[null,"ZYDV100-24S24 ","9-36V","24V ",null,"100W ","EOL"]
[null,"ZYDV100-48S12 ","36-75V","12V ",null,"100W","EOL"]
[null,"ZYDV200-24S12 ","18-36V","12V ",null,"200W ","EOL"]
[null,"ZYDV300-48S24 ","36-75V","24V ",null,"300W ","EOL"]
[null,"ZYDV500-24S24 ","18-36V","24V ",null,"500W","EOL"]
["liquid cooled power supply","ZYAV2000W ","360-400V","12V ",null,"2000W ","292x155x40.5",null,"•High voltage DC input\n•Conversion efficiency\n*Input undervoltage protection\n•Over-current and short-circuit protection\n•Over-temperature protection\n•Input and output isolation\n•Support heat dissipation from water-cooled fins\n*Metal base, fully enclosed case"]
[null,"ZYAV2500W ","360-400V","12V ",null,"2500W ","410x155x40"]
[null,"ZYAV3000W ","360-400V","12V ",null,"3000W","410x155x40"]
["DC and AC in one power supply","HP300-220M53V312 ","165Vac～265Vac18-36Vdc "," +5V/30A;+12V/4A;+3.3V/16\nA;-12V/1A",null,"250W","350*95*45",{"v":0.82,"d":"82%"},"ATX Power Supply\nAC/DC Dual Input Power Supply\n• Internal sealing, anti-vibration, moisture-proof, high\nefficiency\n• High reliability\n• Output overcurrent and output short circuit protection\n• Input and output isolation\n* Modular design\n• Working ambient temperature: 40℃ ~ +55℃"]
[null,"EPC153-2","165Vac～265Vac18-36Vdc","+5V/4A",null,"20W","125*70*25",{"v":0.82,"d":"82%"}]
["1500W charger","EPC153-2 ","165Vac～265Vac18-36Vdc ","30V input adjustable",null,"1500W",null,null,"Single-phase AC input, single constant current output\nCharge\n• Maximum charging current 50A\n• High power factor and high efficiency\n* Input overvoltage and output overload protection function\nable\n• Intelligent temperature control circuit\n• CAN bus communication, trickle current, constant current、\nThree constant voltage charging modes\n• Portable design"]
["24V emergency power supply","YJDY24BC01 ","220Vac ","20-30V",null,"3500A",null,null,"\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n防淋雨设计\n• 交流220V输入，20V～30Vdc输\n出最大峰值电流≥3500A\n• 启动次数： 以启动588kW发机\n机为例，环境温度+50℃情况\n下启动38次；环境温度-40℃情\n况下启动32次\n• -40℃情况下，恒流20A放电，\n持续时间1h42min\n• 常温充电时间50min；-40℃充\n电时间1h20min\n• 适用于应急启动采用24V直流启\n动的陆军装备\n40℃~+55℃\n启动次数：38次\nНепромокаемая конструкция\n* Вход переменного тока 220 В, выход 20 В ~ 30 В постоянного тока\nМаксимальный пиковый ток ≥3500A\n• Количество запусков: для запуска генератора мощностью 588 кВт\nВозьмем, к примеру, машину, температура окружающей среды в которой составляет +50℃\nЗапустите 38 раз; температура окружающей среды -40℃.\nВ этом случае начните 32 раза\n• При температуре -40℃, постоянный ток разряда 20А，\nПродолжительность 1 час 42 минуты\n• Время зарядки при комнатной температуре составляет 50 минут; зарядка при температуре -40℃\nВремя включения 1 час 20 минут\n• Подходит для аварийного запуска при напряжении 24 В постоянного тока.\nДинамичное армейское снаряжение\n40℃~+55℃\nКоличество запусков: 38 раз"]
["power supply for telecom","EPC600-48T3M","48Vdc ","28V/8A/150mV\n12V/20A/120mV",null,null,"Φ252*52mm",{"v":0.9,"d":"90%"}]
[null,"EPC1K-220S48","220Vac","48V/20A/150mV",null,"1000W","266*120*60mm",{"v":0.91,"d":"91%"}]
["Power filter","ESL220-3AW ","220Vac ","3A ",null,null,"70*33*29",null,"• Military power filter\n• According to CE102 conductivity in GJB151A and GJB152A\nDevelopment of startup requirements\n* Solve the electromagnetic interference problem of switching power supplies and inverters\n• Excellent performance of common mode and differential mode insertion loss\n• Excellent low frequency performance\n• Internal potting, anti-vibration, moisture-proof\n• Can be designed based on different insertion loss, working current and voltage、\nCustomized requirements for structure size and terminal connection method\n• Working shell temperature range: -40 ℃ ~ +105 ℃"]
[null,"ESL220-6AT ","220Vac ","6A ",null,null,"75*51*29"]
[null,"EFT220-4BW ","220Vac ","4A ",null,null,"40*50*21"]
[null,"EFL50H-5A ","50Vdc ","5A ",null,null,"70*33*29"]
[null,"EFL50H-10A ","50Vdc ","10A",null,null,"70*33*29"]
["rectifier","ZYR4850H-1U","90-300Vac/18A","42-58Vdc",null,"2900W","L281×W105×H40.","90%+","• Universal AC input voltage range (90VAC-300VAC), output voltage: 42-58VDC\n• Operating temperature range -40℃ ~ +75℃\n• Active load sharing\n*Advanced internal control"]
[null,"ZYR4875H-1U","90-300Vac/25A","42-58Vdc",null,"4000W","L281×W105×H40.","90%+"]
[null,"ZYHTP48400H9C1D1","90-300Vac","42-58Vdc/400A",null,"24000W","L389.1×W482.6×H394.3",null,"•Wide single-phase input range (90VAC-300VAC)\n•Rectifier module operating temperature: -40°C to +75°C\n•High power density\n•THD:≤5%\n•Intelligent control device\n•RoHS compliant\n•TCP/IP, RS232/RS485 communication"]
[null,"ZYTP48400H7C1D1","90-300Vac","42-58Vdc/400A",null,"24000W","L450.0×W482.6×H390.0"]
[null,"ZYTP48150H3C1D2","90-300Vac","42-58Vdc/150A",null,"8700W","L350.0×W482.6×H132.0"]
[null,"ZYTP48350H4C1D1","90-300Vac","42-58Vdc/350A",null,"20000W","L350.0×W482.6×H177.0"]
[null,"ZYTP48600","90-300Vac","42-58Vdc/600A",null,"35000W","L388.5×W584×H263.5"]
[null,"ZYTP48200H5C1D2","90-300Vac","42-58Vdc/200A",null,"116000W","L330.0×W482.6×H218.0"]
["power supply -19\" 2U","EPC5K-220S48M ","220Vac ",null,null,"5000W"]
[null,"EPC4K-220S36M ","220Vac ",null,null,"4000W"]
[null,"EPC4K-220S48T ","220Vac ","48V/80A",null,"4000W","482.6*450*88",{"v":0.92,"d":"92%"}]
[null,"EPC4K-220S36T ","220Vac ","36V/110A",null,"4000W","482.6*450*88",{"v":0.92,"d":"92%"}]
["power supply -19\" 3U","EPC5K-380S48M ","380Vac ",null,null,"5000W "]
[null,"EPC6K-380S48M ","380Vac ",null,null,"6000W"]
["power supply -19\" 4U","EPC4K220M ","AC input 220V ","220Vac",null,"2500W ","482.6*420*177"]
[null,null,"electrical panel input28V ","28Vdc",null,"500W"]
[null,null,"battery input24V "]
["universal power supply -10 output","EPC500-6590A ","AC input220V ","10output",null,"500W","330*295*65",null,"• Waterproof design\n* Dual AC inputs: NETWORK and oil\ninput\n• 10 outputs, modular design, dual redundancy\nSpare backup\n• Soft transfer technology\n• High power factor\n• High efficiency\n• Working ambient temperature: -40℃ ~ +55℃\n* Electromagnetic compatibility: Comply with GJB151B-2013"]
[null,null,"Generator Output 220V "]
["VRM series","BAX100-12-0V8-CTR","9~15VDC","0.5~1.2V",null,"42~600W","SMD",{"v":0.905,"d":"90.50%"},"Non-isolated DC-DC converter\nComplies with IEC/UL/EN6268-1\nSupports remote on/off\nSwitching frequency up to 1100 kHz\nSMD packaging"]
[null,"BAX100-12-0V8-PWR","9~15VDC","0.5~1.2V",null,"42~600W","SMD",{"v":0.905,"d":"90.50%"}]
[null,"BAX80P54D6V7GSG","40~60VDC","5~7.5V",null,"450W","SMD",{"v":0.976,"d":"97.60%"}]
[null,"BAX80P54D13V5GSG","40~60VDC","10~15V",null,"1000W","SMD",{"v":0.981,"d":"98.10%"}]
[]
["performer","ivan wang",89163870458,"WhatsApp"]